Bird Calls

(a) (b)

(c) Figure 3: Comparison of several TFRs of a portion of the bird song of a Cerulean Warbler (Dendroica cerulea) [6]. The sample rate was 16 kHz. (a) Spectrogram computed using a short (64-sample) Hamming window. (b) Spectrogram computed using a long (128-sample) Hamming window. (c) AOK TFR of volume ff = 4 [5].